***Township of Mount Olive Office of the Fire Marshal*** *204 Flanders-Drakestown Rd. PO Box 450 Budd Lake, NJ 07828 (973)691-0900 x7337*

***APPLICATION FOR ONE- & TWO-FAMILY DWELLINGS***

***CERTIFICATE OF SMOKE DETECTOR AND CARBON MONOXIDE***

***ALARM COMPLIANCE IN ACCORDANCE WITH NFPA 74 AND 720***

**You MUST pay your taxes to one of these towns in order to use this form:**

**BUDD LAKE, FLANDERS, HACKETTSTOWN, CHESTER BORO or ALLAMUCHY**

*DATE: \_\_\_\_\_*

*NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ PHONE NO.*

*STREET ADDRESS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*CITY****, ZIP****\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*REALTOR’S NAME: \_\_\_\_\_\_\_\_*

*PHONE NO.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

***Smoke detectors and carbon monoxide detectors must be installed prior to inspection. (See attached form for locations of smoke detectors & carbon monoxide detectors).***

***Your fee of $45.00 pays for the cost of the inspection.***

***\*\*\*Any re-inspections for smoke detectors or carbon monoxide detectors will be an additional $10.00. Fees are paid prior to inspection.***

***\*\*\*All fees are to be paid by check, money order, or exact cash.***

 **\*\*\**MAKE CHECKS PAYABLE TO THE TOWNSHIP OF MT. OLIVE\*\*\****

*Please complete and return this form as soon as possible after you find out your settlement date.*

*Signature of Owner: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Print Your Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

**EFFECTIVE JANUARY 1, 2019 - SMOKE DETECTORS**

5:70-4.19 Smoke alarms for one and two family dwellings; carbon monoxide alarms and portable fire extinguishers

1. In one and two family or attached single family dwellings subject to the requirements of N.J.A.C. 5:70-2.3, smoke alarms shall be installed as follows:
2. The smoke alarms required in (a) above shall be located and maintained in accordance with NFPA 72.

 1. The alarms shall not be required to be interconnected.

 (c)**Ten-year sealed battery-powered single**

 **station smoke alarms shall be installed**

 **and shall be listed in** **Accordance with**

 **ANSI/UL 217, incorporated herein by**

 **reference**. However, A/Cpoweredsingle or Multiple-station smoke alarms installed

 **as** part of the originalconstruction or rehabilitationprojectshall not be replaced with battery

 operated smoke alarms.

1. A/C powered smoke alarms shall be accepted as meeting the requirements of this section.

**PLACEMENT OF SMOKE DETECTORS FOR ONE**

**AND TWO FAMILY RESIDENCES**

The New Jersey State Uniform Safety Act, N.J.S.A.52:27D-198.1 states: a structure used or intended to be used

for residential purposes by not more than two households, shall have a smoke-sensitive alarm device on each

level of the structure and outside each separate sleeping area in the immediate vicinity of the bedrooms and

located on or near the ceiling in accordance with the National Fire Protection Association Standard No. 74-1984. The smoke sensitive device shall be tested and listed by a product certification agency recognized by the Division of Fire Safety.

**WHERE TO PLACE SMOKE DETECTORS**

**Basement area:** The basement smoke detector shall be installed in the basement, within 10 feet of the stairway. The detector shall not be located in the stairway. If installed on an open joists ceiling, the detector shall be placed on the bottom of the joists. For finished ceilings see note below. Living area and/or First Floor: The living area smoke detector shall be installed in the living room and/or near the stairway leading to the upper level. The detector shall not be located in the stairway.

**Bedroom areas:** The bedroom areas smoke detector shall be located in the hall of area outside the bedrooms,

within 10 feet of any bedroom door. In units with more than one bedroom area or with bedrooms on more than one floor, a detector is required within 10 feet of each bedroom.

**Attic area:** Finished attics only. The attic area smoke detector shall be located in the attic near the stairway from the floor below. The detector shall be placed as indicated in note below. Remember if there is a bedroom in the attic the detector must be within 10 feet of the bedroom door.

**NOTE:** Smoke detectors shall be mounted on the ceiling at least 4 inches from the wall or on the wall with the top of the detector not less than 4 inches or more than 12 inches below the ceiling at its highest point. Smoke detectors shall have a low battery warning and test button for easy testing and maintenance. Should you have any questions regarding the placement or testing of detectors please do not hesitate to call our office at (973)691-0900 x7326.

**CARBON MONIXIDE ALARM**

2-1 1.2 A carbon monoxide alarm or detector should be centrally located outside of each separate sleeping area within 10ft. of the bedrooms. Each alarm or detector should be located on the wall, ceiling, or other location as specified in the installation instructions that accompany the unit.

**REQUIREMENTS FOR THE TYPE AND PLACEMENT OF THE**

**EXTINGUISHERS ARE AS FOLLOWS:**

1. At least one portable fire extinguisher shall be installed in all one- and two-family dwellings (except seasonal rental units) upon change of occupancy.

2. The extinguisher shall be listed, labeled, charged, and operable;

3. The size shall be no smaller then **2A:10B:C**, rated for residential use and weigh no more than 10lbs.

4. The hangers or brackets supplied by the manufacturer must be used;

5. The extinguisher must be located within 10 feet of the kitchen and located in the path of egress.

6. The top of the extinguisher must not be more than 5 feet above the floor;

7. The extinguisher must be visible and in a readily accessible location, free from being blocked by furniture,

storage, or other items;

8. The extinguisher must be near a room exit or travel path that provides an escape route to the exterior;

9. The extinguisher must be accompanied by an owner’s manual or written information regarding the

operation, inspection, and maintenance of the extinguisher, and

10. Lastly, the extinguisher must be installed with the operating instructions clearly visible. New fire extinguishers are not required to be serviced and tagged, as long as the seller or agent can provide proof of purchase or receipt.

**